(footprint "Screw_terminal_on_board" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5A19A430)
  (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
  (tags "Through hole socket strip THT 1x06 2.54mm single row")
  (attr through_hole)
  (fp_text reference "REF**" (at 6.3 -1.7) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp d94fd095-7a6e-4e48-86fc-cdfac8e8598a)
  )
  (fp_text value "Screw_terminal_on_board" (at 6 49.2) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 1e2bba13-d127-4ce7-8b02-2883c591f992)
  )
  (fp_text user "${REFERENCE}" (at -2.3 27.6 90) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 6c1c300e-2a47-4ea2-8d52-97571814b130)
  )
  (fp_rect (start 0 0) (end 13.6 47.6) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 3ac4331f-a83f-4965-bc80-409761b5181b))
  (fp_rect (start 0.8 40.45) (end 12.8 46.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 46a1385f-5f4f-4a9b-9654-a1eddc58ac75))
  (fp_rect (start 0.8 24.45) (end 12.8 30.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 52264727-9037-4d7a-aed1-b9baee9f17c2))
  (fp_rect (start 0.8 0.45) (end 12.8 6.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 7b36b7a4-4ab0-4563-b04f-c98e93a03d62))
  (fp_rect (start 0.8 16.45) (end 12.8 22.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp a8d819dc-ae95-4a2a-9494-403054762a39))
  (fp_rect (start 0.8 32.45) (end 12.8 38.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp e98bfc9f-6bc1-4c93-be33-f26c23001579))
  (fp_rect (start 0.8 8.45) (end 12.8 14.95) (layer "F.SilkS") (width 0.12) (fill none) (tstamp f3f70c84-0575-4986-ae89-1da08e73ce4d))
  (pad "1" thru_hole rect (at 6.8 3.7) (size 3 3) (drill 1.5) (layers *.Cu *.Mask) (tstamp 2a8e52ae-6ffa-4b14-871d-c743e160bdeb))
  (pad "2" thru_hole circle (at 6.9 11.6) (size 3 3) (drill 1.5) (layers *.Cu *.Mask) (tstamp a78d5ed1-9fc8-47c8-8861-16da26adfe15))
  (pad "3" thru_hole circle (at 6.9 19.7) (size 3 3) (drill 1.5) (layers *.Cu *.Mask) (tstamp 5d781fb6-49d3-4061-bf95-7a23a7ac5ec1))
  (pad "4" thru_hole circle (at 6.8 27.6) (size 3 3) (drill 1.5) (layers *.Cu *.Mask) (tstamp 94dbc264-1b26-403f-bbbe-3770ea99faa2))
  (pad "5" thru_hole circle (at 7 35.8) (size 3 3) (drill 1.5) (layers *.Cu *.Mask) (tstamp fa40f122-13da-414a-a560-db828fb1be8b))
  (pad "6" thru_hole custom (at 7.1 43.8) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
    (options (clearance outline) (anchor circle))
    (primitives
    ) (tstamp f0bf4302-52ce-45fd-8ac5-ce0a5b7f8539))
  (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
