(footprint "D_Diode_Bridge_KBD" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr through_hole)
  (fp_text reference "REF**" (at -2 -31 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp eab76508-6969-4cf5-bbe5-06367c31abc5)
  )
  (fp_text value "D_Diode_Bridge_KBD" (at 14 -30 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2551f4bc-d4a5-43c7-bbfa-9d7708b2890c)
  )
  (fp_text user "${REFERENCE}" (at 14 4 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp fa414b34-ab91-4a60-bf80-6c6850aa62d3)
  )
  (fp_line (start 27 1) (end -1 1) (layer "F.SilkS") (width 0.12) (tstamp 60df11b7-1dd0-45c7-a583-36b28ec2c772))
  (fp_line (start -1 -27) (end 27 -27) (layer "F.SilkS") (width 0.12) (tstamp 9c6c24d1-3fe6-43c3-b3af-e58180bb3ebf))
  (fp_line (start 27 -27) (end 27 1) (layer "F.SilkS") (width 0.12) (tstamp d784a456-6481-4f20-8f93-07fa33a8d195))
  (fp_line (start -1 1) (end -1 -27) (layer "F.SilkS") (width 0.12) (tstamp f88ba531-9c1e-484c-9193-312cdca36646))
  (fp_rect (start -2 -28) (end 28 2) (layer "Dwgs.User") (width 0.25) (fill none) (tstamp 0d078b94-d74a-44f2-bac7-be1c622d89f1))
  (pad "1" thru_hole rect (at 4.5 -3) (size 9 6) (drill oval 7 2) (layers *.Cu *.Mask) (tstamp 1a3858b8-5ba2-4f2e-9680-f15ed2564a99))
  (pad "2" thru_hole rect (at 4.5 -23.1) (size 9 6) (drill oval 7 2) (layers *.Cu *.Mask) (tstamp 477e2ed4-cda0-4c83-92fc-121407c692b9))
  (pad "3" thru_hole rect (at 21.5 -3) (size 9 6) (drill oval 7 2) (layers *.Cu *.Mask) (tstamp 3c798a46-8f42-4ade-813a-292c093a9cf3))
  (pad "4" thru_hole rect (at 23 -21.7 90) (size 9 6) (drill oval 7 2) (layers *.Cu *.Mask) (tstamp ea6c1606-945d-4b60-a2cc-11657b12a3d4))
)
