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driver converts TTL/CMOS input levels into TIA/EIA-232-F levels. The driver,
hge-generator functions are available as cells in the Texas Instruments LinASIC™ library.

ORDERING INFORMATION
Namine
For
S0IC (DW)

Reel of 2000| MAX232DWR MAX232

SOP (NS) Reel of 2000 MAX232NSR MAX232

PDIP (N) Tube of 25 MAX232IN MAX232IN
Tube of 40 MAX232ID

-40°C to 85°C SoIC (D) Reel of 2500 MAX232IDR MAx232!

Tube of 40 MAX232IDW

SOIC (DW) MAX2321
Reel of 2000 MAX232IDWR

T Package drawings, standard packing quantities, thermal data, symbolization, and PCB design
guidelines are available at www.ti.com/sc/package.
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