ART2003 PIC18Fxxxx Programmer

ATTENTION

This programmer require no external power

and it works in LVP mode, it means that VPP is 5V instead of 13V.

Because that you have to select LVP in FUSES section.
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Hardware configuration in WinPic800
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Also you can use ART2003 hardware config file

LVP selection in FUSES section
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Because it works in LVP mode, you must select allways LVP or you will get errors during programation

