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Simulation Log
Message

@ PROSFICE 7.10.00 (Buid 11532) (C) Labcenter Electronics 1933:2011

@ Losded netist \DOCUME~1\ADMIN\LOCALS “1\TempALISABE1 7. SDF for design C:\Program Files\Labce.
@ 4VR Release 7.75PD buid 12004 for ATMEGAS.

@ Losding HEX fil Termo2ch hex.

@ Read total of 6534 bytes from fle Temo2ch hex' RE[[RI[TRI[RI{RIG

| 4 PC=0:0ACA, [4VR CPU] New DSCCAL valus has changed frequency on 33 16% what s more than recommen 0.000160500s L A IS
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ATHEGAS Message

BUTTON @ 1515 Reease 7.10.00 (B 12325 €] LaboerterElctoics 1590- 2011

DS 18820
o otkroozy || @ Source code buid completed OK.

ERLSEKTIN02Y 1@ Conpling desn C\Program FieLaboentrElecoic Pt 7 ProessionshSAMPLES\TERMOema2 DSN.

@ Netist compilstion completed OK.

@ Netist lnking completed OK.

@ Patiion analysis completed DK.

@ Simuiating partiion [ESACD00]

@ PROSFICE 7.10.00 (Buid 11532) (C) Labcenter Electronics 1933:2011

@ 4VR Release 7.75PD buid 12004 for ATMEGAS.
@ Losding HEX fil Termo2ch hex.
@ Read total of 6534 bytes from fle Temo2ch hex'

@ Losded netist \DOCUME ~1\ADMIN\LOCALS “1\TemphLISABET7.SDF for design C:\Program Fies\Labcenter Elechionics\Proteus 7 ProfessionshSAMPLES\TERMO2\erm.

| 44 PC=040ACA, [AVR CPU]New DSCCAL valug has changed frequency on 33.16% what is more than recommended 2%
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