{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":64,"n_cols":4,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[null,"Наименование","замена","количество"]
[null,"Индикаторы 3631 (3 сегмента общий катод)",null,2]
[null,"светодиоды",null,6]
[null,"тактовая кнопка",null,6]
[null,"кварц 16МГц",null,1]
[null,"Предохранитель 5А",null,1]
[null,"LM7805",null,1]
[null,"LM7812",null,1]
[null,"74HC4052",null,1]
[null,"1N4733A (5,1V / 1Вт)",null,1]
[null,"LM324",null,1]
[null,"IRF630","IRF640 или IRF540N",2]
[null,"1N4148",null,11]
[null,"2N7002",null,7]
[null,"BZT52C5V1 (5,1V / 0,5Вт)",null,2]
[null,"MCP4011-202E (2кОм)",null,2]
[null,"FR152",null,1]
[null,"ATMega32 (TQFP)",null,1]
[null,"Энкодер c кнопкой",null,2]
[null,"Реле 12В*10А (1С)",null,1]
[null,"Терморезистор (с отриц) NTC",null,1]
[null,"C945","BC847",2]
[null,"2SA7338","BC857",1]
[null,"КТ815В","BD137 или BD139",1]
[null,"1N4007",null,1]
[]
[null,"РЕЗИСТОРЫ"]
[null,"0,15 Ом * 15Вт (цементный)",null,1]
[null,"2,2 Ом",null,1]
[null,"К10",null,10]
[null,"К27",null,8]
[null,"1К",null,4]
[null,"1К5",null,2]
[null,"10К",null,2]
[null,"2К2",null,1]
[null,"2К7",null,2]
[null,"3К3",null,4]
[null,"56К",null,4]
[null,"20К",null,2]
[null,"100K",null,2]
[]
[]
[]
[null,"КОНДЕНСАТОРЫ"]
[null,"18pF",null,2]
[null,"220pF",null,1]
[null,"1n",null,2]
[null,"100n",null,5]
[null,"1uF","можно электролит",1]
[null,"2,2uF","можно электролит",4]
[null,"4,7uF","можно электролит",1]
[null,"10uF","можно электролит",4]
[]
[null,"2,2uF*100V",null,1]
[null,"10uF*6,3V",null,1]
[null,"22uF*50V",null,1]
[null,"47uF*16V",null,1]
[null,"220uF*16V",null,1]
[]
[]
[null,"ИНДУКТИВНОСТЬ"]
[null,"20uH",null,1]
[null,"1uH",null,2]
[null,"4100uH (4,1mH)",null,1]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}