DSO Shell DSO150 Oscilloscope DIY Kit
http://www.jyetech.com/Products/LcdScope/e150.php
DSO150  Version 15001K
http://accudiy.com/index.php?main_page=product_info&cPath=3_10&products_id=204
(Version 15001K  15002K  15003K)
Forum   DSO Shell
http://www.jyetech.com/forum/viewforum.php?f=19&sid=b9287cdbdeb5841f87dc3cecd57c7980
DSO150 это улучшенная версия  -  DSO138      Documents 
Чувствительность DSO150 Shell была расширена в обоих направлениях и выше и шире, чем DSO138. 

Он достигает 5mV / дел --- 20V / дел в то время как DSO138 только 10 мВ / дел --- 5V / дел.

Firmwares Source codes - исходники DSO138
http://www.jyetech.com/Products/LcdScope/DSO138_SourceCodes_v037.rar  

Исходные коды также доступны, чтобы позволить пользователю добавлять свои собственные функции.
DSO Shell DSO15001K Digital Oscilloscope DIY Kit
Main Features:
● Vertical position adjustable with indicator
● Adopts flexible firmwares with user-friendly interface, easier to operate
● Waveform storage and playback
● 6 triggering modes
● Complete measurement markers and signal characteristics
● Rotary encoder
Specification:
● ARM Cortex-M3 processor (STM32F103C8)
● Display: 2.4 inch color TFT LCD display resolution: 320 x 240
● Analog broadband: 0 - 200KHz
● Maximum sampling rate: 1Msps 12 bit
● Sampling buffer depth: 1024Bytes.
● Sensitivity error: less than 5 percent
● Maximum input voltage: 50Vpk (1X зонд)
● Coupling mode: DC, AC, GND
● Triggering mode: auto, normal, single
Vertical

Number of Channel: 1

Analog Bandwidth: 0 - 200KHz                   
Sensitivity: 5mV/Div - 20V/Div

Sensitivity error: < 5%

Resolution: 12-bit

Input Impedance: 1M ohm /20pF
Maximum Input voltage: 50Vpk

Coupling: DC, AC, GND
Horizontal

Max Real-time Sampling Rate: 1Msps

Timebase: 10us/Div - 500s/Div

Record Length: 1024
Trigger

Trigger Modes: Auto, Normal, Single

Trigger Types: Rising/falling edge

Trigger Position: 1/2 of buffer size fixed
Power Supply

9V DC (8 - 10V acceptable)

Supply Current: 120mA @ 9V (8-10 В)
главная Размер Доски: 94*65 мм/3.7 * 2.56in

аналоговая Плата Размер: 65*47 мм/2.56 * 1.85in

Размер экрана: 52*40 мм/2 * 1.57in
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