(footprint "Transformer_Toroid_Tapped_Horizontal_D9.0mm_Amidon-T30" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5A030845)
  (descr "Transformer, Toroid, tapped, horizontal, laying, Diameter 9mm, Amidon, T30,")
  (tags "Transformer Toroid tapped horizontal laying Diameter 9mm Amidon T30 ")
  (attr through_hole)
  (fp_text reference "REF**" (at 9.5 -9) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp c0e13872-bc74-4ae4-96b5-d0bb6c5e7c56)
  )
  (fp_text value "Transformer_Toroid_Tapped_Horizontal_D9.0mm_Amidon-T30" (at 7 15) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 9591750f-dbc8-4511-8e55-73ad72355b67)
  )
  (fp_text user "${REFERENCE}" (at 9.5 -9) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dbb14735-c2e7-4cee-90a6-fce8b67a20ef)
  )
  (fp_circle (center 5.5 -3) (end 5.5 -4.4) (layer "F.SilkS") (width 0.12) (fill none) (tstamp 0edc2277-6aba-4170-bdd0-ef82ba0b716e))
  (fp_circle (center 5.5 -3) (end 12.5 -3) (layer "F.SilkS") (width 0.12) (fill none) (tstamp bb14718e-ee49-4728-af26-7b8b2c787e11))
  (fp_circle (center 5.5 -3) (end 19 -3) (layer "F.CrtYd") (width 0.05) (fill none) (tstamp 2f523a69-4223-4f55-8235-e66c29d806c2))
  (fp_line (start 3 3) (end 5.4 -1.4) (layer "F.Fab") (width 0.1) (tstamp 00891628-4ab0-4dd5-99e4-37076499b983))
  (fp_line (start 4.3 -2.2) (end 1 2) (layer "F.Fab") (width 0.1) (tstamp 088f62a0-b965-4576-9306-a19c31dbab44))
  (fp_line (start 10 2) (end 7 -2.5) (layer "F.Fab") (width 0.1) (tstamp 0a4d0ba7-66c1-4382-a3a3-95292f566337))
  (fp_line (start 4.7 -1.7) (end 3 3) (layer "F.Fab") (width 0.1) (tstamp 150d45ae-af3f-4668-ba20-01e72967678f))
  (fp_line (start -1 -0.7) (end 4.3 -2.2) (layer "F.Fab") (width 0.1) (tstamp 17a73a02-e8b0-4db0-9919-aef0cdf4d496))
  (fp_line (start 6.7 -2) (end 10 2) (layer "F.Fab") (width 0.1) (tstamp 1b12eba2-cfca-4c59-a4b9-86e0c5a75bff))
  (fp_line (start 8 3) (end 6.7 -2) (layer "F.Fab") (width 0.1) (tstamp 30aad4aa-36d6-4bff-8ac1-3f9666a62b68))
  (fp_line (start -1 -5.1) (end 4.1 -3.7) (layer "F.Fab") (width 0.1) (tstamp 325c703f-f2cd-4f53-989e-6d5a3fd0c06e))
  (fp_line (start 7 -3.5) (end 12 -4) (layer "F.Fab") (width 0.1) (tstamp 381a489b-22bd-4a4f-8179-7ec770c8e048))
  (fp_line (start 9 -9) (end 6.5 -4.2) (layer "F.Fab") (width 0.1) (tstamp 39e23f5f-6ee0-47ec-b99e-a11da5d7dc95))
  (fp_line (start 5.4 -1.4) (end 5.9 4) (layer "F.Fab") (width 0.1) (tstamp 42006068-4147-4015-8646-abcbb6432726))
  (fp_line (start 1 2) (end 4.7 -1.7) (layer "F.Fab") (width 0.1) (tstamp 4ed9b1ba-2875-4961-bdc2-36f3cadd7f8c))
  (fp_line (start 4.1 -3.7) (end 1 -8) (layer "F.Fab") (width 0.1) (tstamp 56f30464-be92-4da7-b979-513f2ffdf75b))
  (fp_line (start 6.1 -1.6) (end 8 3) (layer "F.Fab") (width 0.1) (tstamp 635bebe3-14a0-4734-981f-f5b6030cdbb2))
  (fp_line (start 6.5 -4.2) (end 11 -7) (layer "F.Fab") (width 0.1) (tstamp 6b11a9a4-621d-4e0d-9a49-ea2dabd6ba6d))
  (fp_line (start 5.9 -10) (end 6 -4.5) (layer "F.Fab") (width 0.1) (tstamp 88a157cc-4e57-42c2-a4de-f3cf4c6a03f9))
  (fp_line (start 11 -7) (end 7 -3.5) (layer "F.Fab") (width 0.1) (tstamp 932231ad-9ee8-46d2-9c3b-de1a2baa023d))
  (fp_line (start 4.5 -10) (end 5.3 -4.6) (layer "F.Fab") (width 0.1) (tstamp 993980ed-dfa2-4cd4-bf17-6fdf5b710fb4))
  (fp_line (start 6 -4.5) (end 9 -9) (layer "F.Fab") (width 0.1) (tstamp a1d1591b-2957-49c6-bb4f-cbfaf99c9251))
  (fp_line (start 1 -8) (end 4.7 -4.3) (layer "F.Fab") (width 0.1) (tstamp aa7b65b7-952d-45b2-8b82-5976d7c7b22b))
  (fp_line (start 5.3 -4.6) (end 5.9 -10) (layer "F.Fab") (width 0.1) (tstamp b262f3c0-91cf-4653-8581-276a9c1c0013))
  (fp_line (start 7 -2.5) (end 12 -4) (layer "F.Fab") (width 0.1) (tstamp ca227d92-57e3-4323-8cdd-9e1950ae405f))
  (fp_line (start 5.9 4) (end 6.1 -1.6) (layer "F.Fab") (width 0.1) (tstamp cae4011e-ca3f-417f-937b-6e305a918844))
  (fp_line (start 4.7 -4.3) (end 4.5 -10) (layer "F.Fab") (width 0.1) (tstamp d5e5d792-c346-42df-9b19-3baf38f67606))
  (fp_circle (center 5.5 -3) (end 7 -3) (layer "F.Fab") (width 0.1) (fill none) (tstamp 91868267-27f5-4779-b007-03c6324b7927))
  (pad "1" thru_hole circle (at -9 8) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 1d754429-b201-4e50-b553-30e8f70492c6))
  (pad "2" thru_hole circle (at 5.5 13) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 4cc1da9d-c229-4844-95b6-d7a813c0403f))
  (pad "3" thru_hole circle (at 20 8) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp d69fe1e7-46b2-4705-a1fc-f72fdd9a4fd5))
  (pad "4" thru_hole circle (at -9 -12) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 766e36d6-6706-47a1-ab40-cf60ff8fe120))
  (pad "5" thru_hole circle (at 5.5 -19) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 16ca3c75-4b4d-4f56-b682-6506bf749a8c))
  (pad "6" thru_hole circle (at 20 -12) (size 2 2) (drill 1) (layers *.Cu *.Mask) (tstamp 4e24c877-8ff1-4a48-8820-e476f2405736))
  (model "${KICAD6_3DMODEL_DIR}/Transformer_THT.3dshapes/Transformer_Toroid_Tapped_Horizontal_D9.0mm_Amidon-T30.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
