USBASP USBISP/AT89S52/AVR/STC/24CXX/ATMEGA STC Programmer Support USB To TTL
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Detailed features:
Overcurrent protection with high performance 500mA resettable fuse to protect your computer motherboard.
USB-powered port 500 mA resettable fuse to prevent damage to the computer USB port. When the output current greater than 500 mA (overcurrent or short-circuit), the self-recovery fuse will immediately cut off the current, the protection of computer motherboards! Resettable fuse will automatically return to normal state, when the lifting of the short-circuit programming can continue normal use

Multi-function:
Support of AT89S51 AT89S52 online download
Online download support for common AVR microcontroller (ATMEGA series)
Support for online download STC Series MCU / SST Series / Philips
Replace PL2303 board of nine brush machine function can be used for USB to TTL board
Can make USB to serial port for serial communication function
 

System Support:Windows XP,Windows7.
The joint use of USB male, can be plugged directly into the computer's USB port, you can also add a USB extension cable into your computer USB port.
On the chip programming, the download cable directly to the target board power supply to the target board not to access any power.If the user is not using the download cable powered interface VCC disconnected.
 

Support chips:
 

AT89S51  AT89S52

ATMEGA8   ATMEGA16   ATMEGA32   ATMEGA64ATMEGA128  ATMEGA8515 ATMEGA8535ATMEGA48ATMEGA88   ATMEGA168

24C01、24C02、24C04、24C08、24C16、24C32、24C64、24C128、24C256、24C512、24C1024.

24LC01、24LC02、24LC04、24LC08、24LC16、24LC32、24LC64、24LC128、24LC256、24LC512、24LC1024.

STC Series：STC89C51RC、 STC89C52RC、STC89C53RC、STC89C54RD+、STC89C55RD+、STC89C58RD+、STC89C510RD+、 STC89C512RD+、STC89C513RD+、STC89C514RD+、STC89C516RD+、STC89C58RD、 STC89C561RD etc. 

STC12C1052、STC12C2052、STC12C3052、STC12C4052、 STC12C5052、STC12C1052AD、STC12C2052AD、STC12C3052AD、STC12C4052AD、 STC12C5052AD  etc.
STC11F01、STC11F02、STC11F03、STC11F04、STC11F05、STC11F01E、STC11F02E、STC11F03E、STC11F04E、STC11F05E   etc.

  STC10F02、STC10F04、STC10F06、STC10F08、STC10F010、STC10F012  etc.

STC12C5A60S2 Series

STC12C5608AD Series
